**For Bullfrog Spa Owners Using the Silk Balance Water Care System**

**Getting Started:**

*If using a brand-new spa* – Set pH and alkalinity of your water (check using test strips), this can take 2 to 3 days. Then, add 2 oz SilkBalance for your initial use.

*If just starting Silk Balance in your previously used spa* – first utilize CleanStart to fully clean out your spa’s lines and plumbing. This will completely clean your spa and restore the plumbing to factory conditions (instructions for CleanStart are located on the back of the bottle.) After using CleanStart, refill your spa and set the pH and alkalinity, then add 3 oz SilkBalance for your initial use.

**Chemical Usage:**

* Add one Teaspoon of potassium peroxymonosulfate (OxyBrite) every use of your spa.
* Add one tablespoon of chlorine every week.
* Add 2 ozs of SilkBalance every week.

**Draining your spa:**

Drain your water one month after installation/initial fill to remove factory laminates. After that, we recommend draining every six months (twice a year) for optimal enjoyment and water quality.

**Filter Cleaning:**

We recommend cleaning your filters monthly with high-pressure water (no dish soap.) A horsehair brush can be used to remove large debris. We also recommend soaking your filters for 24 hours in GLB Filter Fresh once a year, or using LeisureTime Instant Cartridge Clean.